	Acceptance protocol for memory card replacement
	

	i650 motec ES-IO
	



Acceptance protocol for i650 motec ES-IO device-replacement

This acceptance protocol is only designed for component replacement without change of the safety functionality.

General

	Date
	[bookmark: Text2]01.01.2026

	Carried out by
	[bookmark: Text3]     




Machine description

	Manufacturer
	[bookmark: Text5]     

	Machine / type / number
	[bookmark: Text4]     

	System / system part
	[bookmark: Text6]     

	Name of axis
	     




Execution

	Step
	Description
	Actual status / value

	1
	Switch on drive controller
	

	2
	Read serial number of drive controller (0x2000:002) or from housing
	[bookmark: Text18]     

	3
	Read CRC of safe parameter set (0x2115:002)
	     

	If the index specified in step 3 can no longer be read out, use the values from the commissioning acceptance protocol for i650 motec ES-IO.

	4
	Read firmware version of ES-IO (0x212C:001)
	     

	5
	Switch off drive controller
	

	6
	Replace device
	

	7
	Switch on drive controller
	

	8
	- Transfer application to drive controller
- Reset the parameter set in the device and transfer safe parameter set to the drive controller
	

	9
	Read CRC of safe parameter set (0x2115:002)
	     

	10
	Compare the CRC value with the value of step 3. 
	

	11
	Are the CRC values identical?
(This is the safety-relevant check!)
	Please tick
	[bookmark: Kontrollkästchen1]|_| yes

	
	
	
	[bookmark: Kontrollkästchen2]|_| no



Countersignature

The 'service engineer'

hereby confirms that the above-described tests and checks were carried out properly by skilled personnel.

	Date
	Name
	Company / department
	Signature
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